	  

Country
  

EEC
  

G.B.
  

BELGIUM
  

HOLLAND
  

WORLD
  

TEMP
  

RANGE
MODE

1

2

3

4

5

6

7

DOOR / BONNET / BOOT / KEY ON ALARM CYCLES 

  

3

  

8

  

3

  

3

  

3

  

X

  

31

VOLUMETRIC AND ANTI-TILT ALARM CYCLES

  

3

  

8

  

3

  

3

  

3

  

X

  

31

CABLE CUT ALARM CYCLES 

  

3

  

12.

  

3

  

3

  

3

  

X

  

31

TOTAL ALARM CYCLES

  

10

  

24

  

12

  

12

  

10

  

X

  

255

PAUSE BETWEEN ALARM CYCLES

  

6 seconds

  

6 seconds

  

4 seconds

  

6 seconds

  

6 seconds

  

X

  

31 seconds

SIREN ALARM TIME (S)

  

26 seconds

  

26 seconds

  

26 seconds

  

26 seconds

  

26 seconds

  

X

  

255 seconds

SIREN POWER

110 DBA

110 DBA

110 DBA

114 DBA

110 DBA

X

255 DBA

ACOUSTIC SIGNAL

  

CONTINUOUS

  

CONTINUOUS

  

CONTINUOUS

  

CONTINUOUS

  

CONTINUOUS

  

X

  

N/A

SIREN SOUND

 MODULATED

 MODULATED

 MODULATED

 MODULATED

 MODULATED

X

N/A

SIREN FREQUENCY MODULATION

  

2±1 Hz

  

2±1 Hz

  

2±1 Hz

  

2±1 Hz

  

2±1 Hz

  

X

  

20 Hz

SIREN SOUND FREQUENCY

  

1800-3500 Hz

  

1800-3500 Hz

  

1800-3500 Hz

  

1800-3500 Hz

  

1800-3500 Hz

  

X

  

5000 Hz



	Cancelling the procedure. If the rear fog lamp button is not pressed for 10 seconds whilst entering the operating mode, the procedure is aborted; in this case the siren will beep 5 times to warn the operator and the NBC will maintain the previous operating mode.




