Swapping engine mounts


The rear "beaver" panel from the Niki/126 with the engine mount shown after the spot welds have been drilled out.
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The Niki/126 engine mounting bracket welded onto the 500 "beaver" panel, shown here with engine fitted and spring in position.

· Drill out all spot welds holding the engine mounting brackets from both rear panels.

· Work out how high you want your engine to fit, depending on what type of carburettor you want to use.

· Mig weld the Niki/126 bracket in place of the old 500 one.

NB; watch the height of the bracket as it needs to be fitted higher than the top lip would indicate.

(if in doubt, wait until your engine is refitted and mark where it needs to go)

